Tender specifications: Portal SGB 17 Mix 3/1

High quality, especially wear-resistant entrance mat, improved absorption of coarse dirt

Application: Indoor and roofed exterior; normal up to extremely strong frequency, suitable for wheelchairs, overall laying, Static point loading up to 4500 kg per 80 cm²

Stripe profile: aluminum, with scratching edge, sound insulated

Cleaning stripes: Rubber and brush, mix 3/1 (minimum 24 brush profiles each metre of walking depth)

Rubber profiles: serrated lengthways; aluminum profile edges covered; high quality material mix; colour black; slip resistance R 9 according to DIN 51130

Brush: ARWEI three-way brush; brushes on different levels for an improved absorption of coarse dirt, sound insulating, colour black, slip resistance R 13 according to DIN 51130

Connection: ARWEI Special Connectors; therefore easily to roll up, high slip resistance by anti-slip function; modular construction – no wire or cable connections -, each part can easily be replaced on the spot

Height 17 mm  
Stababstand 4 mm: 25 brush profiles each m of walking depth  
Stababstand 6 mm: 24 brush profiles each m of walking depth  
Angle frames in 20 x 20 x 3 mm are available in aluminum, brass or stainless steel.

(\_) 4 mm

(\_) 6 mm

Measurement:

Bar distance:'..........'mm

Walking depth:'..........'mm

Type: ARWEI Portal SGB 17 Mix 3/1

ARWEI-Bauzubehör GmbH

Kalteiche-Ring 48, 35708 Haiger

Tel. +49 (0) 2773 917 880, Fax +49 (0) 2773 917 88 50

E-Mail: info@arwei.de